User Manual

Hermit Crab

Hermit Crub members

Moreno Sardella, master degree student in computer science and engineering

Luca Fochetta, master degree student in computer science and engineering

Dimitar Anastasovski, master degree student in computer science and engineering

Lorenzo Vignati, master degree student in biomedical science and engineering

Paolo Ritter, master degree student in biomedical science and engineering

Summary

[1 – Overview 3](#_Toc506305789)

[2 – Hermit Crab Usage 4](#_Toc506305790)

[2.1 – Required Workspace 4](#_Toc506305791)

[2.2 – Custom Menu and Hermit Crabs placement 4](#_Toc506305792)

[2.3 – Treasure Box 4](#_Toc506305793)

[2.4 – Shell Placement 4](#_Toc506305794)

[2.5 – Usage 4](#_Toc506305795)

[2.6 – Enjoy 4](#_Toc506305796)

[3 – Components Replacement 5](#_Toc506305797)

[3.1 – Battery Replacement 5](#_Toc506305798)

[3.2 – Soap Replacement 5](#_Toc506305799)

# 1 – Overview

On this manual will be explained how to properly use yours Hermit Crab. The package should be composed of:

* 2 Hermit Crabs
* 2 Shells
* 2 Batteries
* 1 Treasure Box
* 1 Custom Menu
* 1 Battery Charger
* 1 Micro-usb cable

# 2 – Hermit Crab Usage

## 2.1 – Required Workspace

In order to properly use the Hermit Crab product you will need a table that is at least 1x1 m.

## 2.2 – Custom Menu and Hermit Crabs placement

The custom menu must be open and put on the table with the white part on top. The Hermit Crabs must be put on a white part of the menu, separated by some centimeters.

## 2.3 – Treasure Box

The Treasure Box must be put next to the menu, with the front side directed to the area where the people would walk. The Box must be closed also to a power point in order to feed it. Then connect the plug.

## 2.4 – Shell Placement

The shell must be put on top of the Hermit Crab “cage” with the higher part on the back of the hermit. Then you must delicately push the shell down until it will be fixed with the cage.

SOME IMAGEs

## 2.5 – Usage

In order to make the Hermit Crab work, you have to turn them to on by the moving the switch placed on the bottom of them to On. Then you to press the button of the Treasure Box placed on the back of it to on.

## 2.6 – Enjoy

Now you have succesfully installed yours Hermit Crab Product. Well Done!

# 3 – Components Replacement

## 3.1 – Battery Replacement

In order to replace the battery of an Hermit Crab you have to possess a battery lp-e8(7.4 V).

To substitute the battery you have to follow those steps:

1. Gently remove the shell from the skeleton.
2. Open up the dome.
3. Remove the wood connector from the battery.
4. Remove/replace the old battery with the new one.
5. Recconect the wood connector being very careful to connect positive pole of the battery with the corresponding one on the wood connector, same must be done for the negative pole.
6. Move the hermit crab arm in position like in figure and then move down the dome.
7. Gently put the shell on the dome ( follow 2.4 – Shell Placement).

## 3.2 – Soap Replacement