User Manual

Hermit Crab

Hermit Crub members

Moreno Sardella, master degree student in computer science and engineering

Luca Fochetta, master degree student in computer science and engineering

Lorenzo Vignati, master degree student in biomedical science and engineering

Paolo Ritter, master degree student in biomedical science and engineering

Dimitar Anastasovski, master degree student in computer science and engineering

Summary

[1 – Overview 3](#_Toc506305789)

[2 – Hermit Crab Usage 4](#_Toc506305790)

[2.1 – Required Workspace 4](#_Toc506305791)

[2.2 – Custom Menu and Hermit Crabs placement 4](#_Toc506305792)

[2.3 – Treasure Box 4](#_Toc506305793)

[2.4 – Shell Placement 4](#_Toc506305794)

[2.5 – Usage 4](#_Toc506305795)

[2.6 – Enjoy 4](#_Toc506305796)

[3 – Components Replacement 5](#_Toc506305797)

[3.1 – Battery Replacement 5](#_Toc506305798)

[3.2 – Soap Replacement 5](#_Toc506305799)

# 1 – Overview

On this manual will be explained how to properly use yours Hermit Crab. The package is composed of:

* 2 Hermit Crabs
* 2 Shells
* 2 Batteries
* 1 Treasure Box
* 1 Custom Menu
* 1 Battery Charger
* 1 Micro-usb cable
* 1 Power supplier

# 2 – Hermit Crab Usage

## 2.1 – Required Workspace

In order to properly use the Hermit Crab product you will need a table that is at least 1x1 m.

## 2.2 – Custom Menu and Hermit Crabs placement

The custom menu must be on the table unfolded, with the white part on top. The Hermit Crabs must be put on the center part of the menu.

## 2.3 – Treasure Box

The Treasure Box must be put next to the menu, with the front side directed to the area where the people will walk. The Box must be closed to a power point in order to supply it. Then connect the plug.

## 2.4 – Shell Placement

The shell must be put on top of the Hermit Crab “cage” with the bigger part on the front of the hermit(see the image). Then you must delicately push the shell down until it will be fixed with the cage.

SOME IMAGEs

## 2.5 – Usage

In order to make the Hermit Crab work, you have to turn them on by moving the switch placed on the bottom of them to On. Then you to press the button of the Treasure Box placed on the back of it to On.

## 2.6 – Enjoy

Now you have succesfully installed yours Hermit Crab Product. Well Done!

# 3 – Components Replacement

## 3.1 – Battery Replacement

In order to replace the battery of an Hermit Crab you have to possess a battery LP-E8(7.4 V).

To substitute the battery you have to follow these steps:

1. Gently remove the shell from the Hermit Crab.
2. Open up the cage.
3. Remove the wood connector from the battery.
4. Remove/replace the old battery with the new one.
5. Recconect the wood connector being very careful to the polarity.
6. Move the hermit crab arm in position like in figure and move down the cage.
7. Gently put the shell on the cage ( follow 2.4 – Shell Placement).

## 3.2 – Soap Replacement